# Config file for x2s3667

#details of the condition

driver_condition = 'He:1.0'
test_gas = 'gas_giant_80_he'
secondary = False
nozzle = True
conehead = True
area_ratio = 5.64
piston = 'lwp-2.5mm'
shock_over_model = True

#fill pressures (in Pa)
nominal_shock_tube_fill = 2000.0
nominal_acc_tube_fill = 0.5

actual_shock_tube_fill = nominal_shock_tube_fill
actual_acc_tube_fill = 0.52

#any notes about the condition

notes = "None."

canny_settings_dict = {}

canny_settings_dict['at'] = {'sigma':2, 'derivative_threshold':0.001, 'post_suppression_threshold':0.08}
# supposedly this is a way to copy dictionaries in Python...
# copy the at dictionary and then add a start time which is past the mechanical noise
canny_settings_dict['at7'] = dict(canny_settings_dict['at'])
canny_settings_dict['at7']['start_time'] = 0.00180
canny_settings_dict['at8'] = canny_settings_dict['at7']
canny_settings_dict['sd'] = {'sigma':2, 'derivative_threshold':1.0, 'post_suppression_threshold':10.0}
canny_settings_dict['st'] = canny_settings_dict['at']
canny_settings_dict['pt'] = {'sigma':3, 'derivative_threshold':0.001, 'post_suppression_threshold':0.07,'start_time':0.00180}
canny_settings_dict['trigbox'] = {'sigma':1, 'derivative_threshold':10.0, 'post_suppression_threshold':100.0,'start_time':0.00150}
